HID touch screen driver installation for CentOS 5_64bit 

(C) 2010 AIM TOUCH TECHNOLOGY CO.,LTD.



==============================================================================
QUICKSTART GUIDE
==============================================================================

I. Installsation guide


1. Open terminal


2. Enter root user
# sudo -s

3. Execute Setup.sh
# sh setup.sh



II. Installation Notes for RS232 touch interface.


1. After finished steps above, please modify X11 driver

   
a. Add the following lines into xorg.conf(located in /etc/X11):


Find "ServerLayout" section, add following line if there is no such setting.


InputDevice 	"HID TOUCH" 


(Note: If your system will not have a mouse, then use "CorePointer" instead of
"SendCoreEvents" in the "ServerLayout" section.)


b. Add the a new "InputDevice" Section as the following if there is no such setting:


Section "InputDevice"

Identifier"HID TOUCH"

Driver "xfhiddrv"

Option "Device" "/dev/ttyS0"

Option "ScreenNo" "0"

Option "Rotation" "0"

Option "SwapY" "0"

Option "AlwaysCore"

Option "UpSound" "0"

Option "DownSound" "0"

Option "AutoRightClick" "1"

EndSection

(Note:In "Device" item, "/dev/ttyS0" may be different depends on which COM port is connected.)


"/dev/ttySx"    x=0,1,..., n (ttyS0 means COM1, you can modify it by this rule) 


c.After modify these settings, please type

#reboot 
to restart X server. 


III. Setup and run Linear Utility:

a. Run linearity utility
      
I. USB HID device
      
#./LinearAp  /dev/hiddevx n
      
II. RS232 device
      #./LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  
      
      
