Touch screen driver installation for Ubuntu 10.04-03 and X11_32 bit

(C) 2010 AIM TOUCH TECHNOLOGY CO.,LTD. 



==============================================================================
RELEASE NOTE
==============================================================================

ubuntu-10.04-0.1

Initial version with tool

ubuntu-10.04-0.2
Initial version driver only

ubuntu-10.04-0.3
Fix right click issue on desktop

==============================================================================
QUICKSTART GUIDE
==============================================================================

I. Installsation guide


1. Open terminal


2. Login as root user
# sudo -s

3. Execute setup.sh

# sh setup.sh


II. Installation Notes for RS232 touch interface.


1. After finished steps above, please modify X11 driver


   a. Add the following lines into xorg.conf(located in /etc/X11):
        
        Find "ServerLayout" section, add following line if there is no such setting.


    	InputDevice 	"HID TOUCH" 


       (Note: If your system will not have a mouse, then use "CorePointer" instead of
         "SendCoreEvents" in the "ServerLayout" section.)


   b. Add the a new "InputDevice" Section as the following if there is no such setting:
   
Section "InputDevice"
        Identifier  "HID TOUCH"
        Driver      "xfhiddrv"
        Option      "Device" "/dev/ttyS0"
        Option	    "ScreenNo"	"0"
	Option	    "SwapY"	"0"
	Option	    "SendCoreEvents"	"true"
EndSection


     (Note:In "Device" item, "/dev/ttyS0" may be different depends on which COM port is connected.)


        "/dev/ttySx"    x=0,1,..., n (ttyS0 means COM1, you can modify it by this rule) 


   c.  After modify these settings, please type
       #reboot 
       to restart X server. 


III. Setup and run Linear Utility:


   a. Run linearity utility
      
I. USB HID device
      #LinearAp  /dev/usb/hiddevx n
      
II. RS232 device
      #LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  
      
      
