Touch screen driver installation for opensuse 11.2 11 and X11 
(C) 2010 AIM TOUCH TECHNOLOGY CO.,LTD.

==============================================================================
QUICKSTART GUIDE
==============================================================================
1. create a xorg.conf from xorg.conf.install
   a. copy xorg.conf.install as xorg.conf
   b. reboot

2. setup xorg driver
   a. decompress xfhiddrv_drv.tar.gz
      #gzip -d xfhiddrv_drv.tar.gz
      #tar xvf xfhiddrv_drv.tar 
   b. Copy xfhiddrv_drv.so to /usr/lib/xorg/modules/input/xfhiddrv_drv.so 

      #cp   xfhiddrv_drv.so /usr/lib/xorg/modules/input/xfhiddrv_drv.so

   c. In the Section "ServerLayout" Add the following line (refer to xorg.conf)

      InputDevice    "HID TOUCH"

   d. Add the following section

      Section "InputDevice"
	   Identifier  "HID TOUCH"
	   Driver      "xfhiddrv"
	   Option      "Device"           "/dev/usb/hiddev0"
	   Option      "ScreenNo"         "0"
	   Option      "Rotation"         "0"
	   Option      "DebugLevel"       "0"
	   Option      "DownSound"        "0"
       	   Option      "UpSound"          "0"
      EndSection

      Ps: if UART, should be Option      "Device"           "/dev/ttySx", x=0,1,2...
   e. Press Ctrl+Alt+Backspace to restart X server. 
   
2. calibration
   a. installation 
      step 1. decompress LinearAp.tar.gz 
         #gzip -d LinearAp.tar.gz
         #tar xvf LinearAp.tar
      step 2. copy linearity utility to /usr/local/bin
         #cp ./LinearAp /usr/local/bin
         
   b. Run linearity utility
      I. HID device
         a. enter root mode.
            $su
             (Keyin your password)
         b. execute program.
         #./LinearAp  /dev/usb/hiddevx n
      
      II. RS232 device
         a. enter root mode.
            $su
             (Keyin your password)
         b. execute program.
            #./LinearAp  /dev/ttySx n
            where x=0,1,2...n, n = 4 or 9 <default>  



      
      
