Touch screen driver installation for Moblin2.1 and X11 

(C) 2006 AIM TOUCH TECHNOLOGY CO.,LTD.

================================
QUICKSTART GUIDE
=====================================

User can select I or II to setup the driver.

I. Using Setup.sh.

1. Open termial

2. sudo -s 
   enter root user

3. sh Setup.sh
   execute script file to setup
   


II. Using Manual setup.       

1. setup xorg driver
   
 a. decompress xfhiddrv_drv.tar.gz
      #gzip -d xfhiddrv_drv.tar.gz
      #tar xvf xfhiddrv_drv.tar 
   
 b. Copy xfhiddrv_drv.so to /usr/lib/xorg/modules/input/xfhiddrv_drv.so 

      #cp   xfhiddrv_drv.o /usr/lib/xorg/modules/input/xfhiddrv_drv.so

   
 c. In the Section "ServerLayout" Add the following line (refer to xorg.conf)

      InputDevice    "HID TOUCH"

   
 d. Add the following section

      Section "InputDevice"
	   Identifier  "HID TOUCH"
	   Driver      "xfhiddrv"
	   Option      "Device"           "/dev/input/event0"
	   Option      "ScreenNo"         "0"
	   Option      "Rotation"         "0"
	   Option      "DownSound"        "0"
       Option      "UpSound"          "0"
      EndSection

   
 e. Press Ctrl+Alt+Backspace to restart X server. 
   

2. calibration
   
a. installation 
      
 step 1. decompress LinearAp.tar.gz 
         #gzip -d LinearAp.tar.gz
         #tar xvf LinearAp.tar
      
 step 2. copy linearity utility to /usr/local/bin
         #cp ./LinearAp /usr/local/bin
         
   
b. Run linearity utility
      
I. HID device
      #./LinearAp  /dev/hiddevx n
      
      
II. RS232 device
      #./LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  



      
      
