Touch screen driver installation for MacOS-10.6.8-Intel CPU.
(C) 2011 AIM TOUCH TECHNOLOGY CO.,LTD.

============How To Get a Command Terminal Window=======================================


To access a "TERMINAL" window under OS X:


You may have a shortcut in the task bar (at bottom of screen) for Applications, or you may not.


If you do, then simply click on the Applications icon in the task bar. ==>Applications ==>Utilities ==>Terminal 


===================================================================================


I. Setup procedures

1. Decompress the driver file and copy the folder to your desktop. 

2. Open the Terminal. 

3. sudo -s and input root password.

4. cd /Users/namexxxx/Desktop/MacOS-R(modify namexxxx to your user name)

5. sh setup.sh
6. Reboot your Mac computer.



II. Do Calibration

1. Open MacOS-R(driver folder) on your desktop

2. double click LinearAp.

3. follow the indicator.



III. Uninstall procedures
== In Terminal Window ==

1. sudo -s and input root password.

2. cd /System/Library/Extensions/

3. rm -R HidTouch.kext

4. reboot your Mac computer.