HID touch screen driver installation for Fedora 12 and X11 
(C) 2010 AIM TOUCH TECHNOLOGY CO.,LTD.



==============================================================================
RELEASE NOTE
==============================================================================

fedora-12-0.1
Initial version with tool

fedora-12-0.2
Initial version driver only

fedora-12-0.3
Modify so to fix right click issue on desktop

fedora-12-0.4
Modify right click repeat issue

==============================================================================
QUICKSTART GUIDE
==============================================================================

I. Installsation guide


1. Open terminal


2. Login as root user
# sudo -s

3. Execute setup.sh
# sh Setup.sh



II. Installation Notes for RS232 touch interface.


1. After finished steps above, please modify X11 driver

   
a. Add the following lines into xorg.conf(located in /etc/X11):
        
        Find "ServerLayout" section, add following line if there is no such setting.

    	InputDevice 	"HID TOUCH" 

       (Note: If your system will not have a mouse, then use "CorePointer" instead of
         "SendCoreEvents" in the "ServerLayout" section.)

   
b. Add the a new "InputDevice" Section as the following if there is no such setting:
   
Section "InputDevice"
        Identifier  "HID TOUCH"
        Driver      "xfhiddrv"
        Option      "Device" "/dev/ttyS0"
        Option	    "ScreenNo"	"0"
	Option	    "SwapY"	"0"
	Option	    "SendCoreEvents"	"true"
EndSection

     (Note:In "Device" item, "/dev/ttyS0" may be different depends on which COM port is connected.)

        "/dev/ttySx"    x=0,1,..., n (ttyS0 means COM1, you can modify it by this rule) 

   
c.  After modify these settings, please type
       #reboot 
       to restart X server. 



III. Setup and run Linear Utility:

   
a. Run linearity utility
      
I. USB HID device
      #LinearAp  /dev/usb/hiddevx n
      
II. RS232 device
      #LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  
      
      
