Touch screen driver installation for Ubuntu-9.04_32bit. 
(C) 2006 AIM TOUCH TECHNOLOGY CO.,LTD.

1. Please copy these 2 files to user directory (e.g. /home/ruby) 

2. Change to user directory "#cd /home/ruby" , then "#sudo -s" to enter root mode

3. Run setup by "#sh setup.sh", then reboot.

4. OK, it's done, the Calibration tool(LinearAp) is installed in "Accessories" of desktop.