Touch screen driver installation for netebook-alpha2 and X11 

(C) 2006 AIM TOUCH TECHNOLOGY CO.,LTD.

=======================
QUICKSTART GUIDE
=================================

User can select I or II to setup the driver.


I.Using Setup.sh.

1. Open termial
2. sudo -s 
   enter root user

3. sh Setup.sh
   execute script file to setup
   


II. Using Manual setup.

1. setup xorg driver

a. decompress xfhiddrv_drv.tar.gz
      #gzip -d xfhiddrv_drv.tar.gz
      #tar xvf xfhiddrv_drv.tar
b. Copy xfhiddrv_drv.so to /usr/lib/xorg/modules/input/xfhiddrv_drv.so 

      #cp   xfhiddrv_drv.o /usr/lib/xorg/modules/input/xfhiddrv_drv.so


c. In the Section "ServerLayout" Add the following line (refer to xorg.conf)

      InputDevice    "HID TOUCH"


d. Add the following section

      Section "InputDevice"
	   Identifier  "HID TOUCH"
	   Driver      "xfhiddrv"
	   Option      "Device"           "/dev/usb/hiddev0"
	   Option      "ScreenNo"         "0"
	   Option      "Rotation"         "0"
	   Option      "DebugLevel"       "0"
	   Option      "DownSound"        "0"
       	   Option      "UpSound"          "0"
      EndSection

   
e. Press Ctrl+Alt+Backspace to restart X server.


2. calibration

a. installation 
      
step1. 
  decompress LinearAp.tar.gz 
         #gzip -d LinearAp.tar.gz
         #tar xvf LinearAp.tar
      
step2. 
  copy linearity utility to /usr/local/bin
         #cp ./LinearAp /usr/local/bin
         
   
b. Run linearity utility
      
I. HID device
      #./LinearAp  /dev/hiddevx n

II. RS232 device
      #./LinearAp  /dev/ttySx n
      where x=0,1,2...n, n = 4 or 9 <default>  



      
      
